{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Welkom","Brongegevens type 4","Versiebeheer"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Welkom","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[]}
[]
["Met behulp van deze tool is het eenvoudig om een OPS-bronbestand \"type 4\" aan te maken vanuit MS-Excel."]
["Vul de benodigde gegevens in, of importeer deze vanuit een ander bestand, en kies vervolgens de optie \"Maak Bronbestand\" uit het \"cell menu\" (rechter muisklik);"]
["of kies de optie \"Schrijf bronbestand naar disk\" uit het \"Maak Bronbestand\" menu op het Add-Ins tabblad."]
[]
["Een OPS-bronbestand moet aan een bepaald format voldoen, zowel qua opbouw als getalsformaat. \"Maak bronbestand\" verzorgt dit en valideert de geldigheid van de ingevulde gegevens."]
["Een bronbestand is geldig voor één component. Meer informatie over het OPS-bronbestand is te vinden in de OPS User Manual, paragraaf 'Emission file'."]
[]
["Klik HIER om de gegevens van de bronnen in te vullen"]
[]
["Voor een correct werkend OPS-bronbestand zijn alle volgende parameters nodig:"]
[]
["Parameter","Omschrijving",null,null,null,"Bereik","Type"]
["snr","volgnummer van de bron",null,null,null,"0 - 9999","integer"]
["x(m)","x-coördinaat van de bron in RDM (meter)",null,null,null,"-9999999 - 99999999 *","long integer"]
["y(m)","y-coördinaat van de bron in RDM (meter)",null,null,null,"-9999999 - 99999999 *","long integer"]
["q(g/s)","bronsterkte (gram/seconde)",null,null,null,"0 - 9999","real number"]
["hc(MW)","warmtecapaciteit van de bron (MegaWatt)",null,null,null,0,"real number"]
["h(m)","hoogte van de bron (meter)",null,null,null,"0 - 20","real number"]
["r(m)","diameter van de bron (meter)",null,null,null,"-999999 - 99999","long integer"]
["s(m)","verdeling van de bronhoogte (meter)",null,null,null,"0 - h(m)","real number"]
["D_stack(m)","schoorsteendiameter",null,null,null,"0.01 -5","real number"]
["V_stack(m/s)","uitstroomsnelheid uit de schoorsteen",null,null,null,"0 - 8.4","real number"]
["Ts_stack(°C)","uitstromendgastemperatuur",null,null,null,-999,"real number"]
["dv","code voor dagelijkse variatie van de emissie",null,null,null,"-999 - 9999","integer"]
["cat","categorie van de bron",null,null,null,"0 - 9999","integer"]
["area","regiocode van de regio waarin de bron staat",null,null,null,"0 - 9999","integer"]
["ps","code voor deeltjesgrootteverdeling",null,null,null,"1 t/m 9999 of -999 t/m -1; 0 = gasvormig","integer"]
["L(m)","lengte van het gebouw",null,null,null,"10 - 105","real number"]
["W/L(-)","breedte/lengte-verhouding van het gebouw",null,null,null,"0.15 - 1","real number"]
["H(m)","hoogte van het gebouw",null,null,null,"0 - 20","real number"]
["O(°)","orientatie van het gebouw",null,null,null,"0 - 180","integer"]
["component","componentnaam (=facultatieve invoer)",null,null,null,"-","text, maximaal 12 karakters"]
["bronomschrijving","omschrijving van de bron (=facultatieve invoer)",null,null,null,"-","text, maximaal 128 karakters"]
[]
["*: Het geldigheidsgebied van de RD-coördinaten beslaat een rechthoekig gebied met x-waarden tussen -7000 en +300000 meter en y-waarden tussen +289000 en +629000 meter."]
["In OPS mogen de x- en y-waarde variëren van -9999999 tot 99999999 meter. Meer informatie:"]
[]
["De geodetische referentiestelsels van Nederland",null,null,null,null,"(§3.2.6 \"Geldigheidsgebied van de definitie RD2000\")"]
[]
["v1.1"]

{"sheet":"Brongegevens type 4","index":1,"n_rows":1,"n_cols":21,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["snr","x(m)","y(m)","q(g/s)","hc(MW)","h(m)","r(m)","s(m)","D_stack(m)","V_stack(m/s)","Ts_stack(°C)","dv","cat","area","ps","L(m)","W/L(-)","H(m)","O(°)","component","bronomschrijving"]

{"sheet":"Versiebeheer","index":2,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["v1.0","2020-10-14","Initiële versie"]
["v1.1","2020-10-20","Range en type van parameter r(m) aangepast in VBA-code"]